Installation and Use of the Briga-jig
The Briga-Jig is an easy, accurate and time-saving system for the installation of wood and composite shingles to the sidewall or roof of a structure.
STEP 1: Begin by first choosing a straight, lightweight ledger board with a desired length, and ripped down to a desired course width.
STEP 2: Using one Briga-jig, insert the retention leg (a) up and behind the previous course of shingles until jig sets tight against butt edge of shingles, just short of the total length of ledger board.
STEP 3: Repeat step two with the second Briga-jig, down the course of shingles, just short of the length of the ledger board.
STEP 4: The ledger board (b) may now be inserted down and onto the shelf created by installed Briga-jigs.  Once shelf is inserted, re-check Briga-jigs to ensure jigs are fully inserted against butt edge of previously installed shingles.
STEP 5: You are now ready to begin shingle installation (c) .  Always remember proper keyway alignment, gaping, and nail patterns.  Course adjustment may be necessary.
STEP 6: When course adjustment is desired, Briga-jigs offer up to a ½-inch adjustment to either gain or lose in course widths, using the scale and adjustment knob on the front of the jig.
STEP 7: Once row or course of shingles is completed, remove ledger board and pull each Briga-jig downward and away until extracted.
[bookmark: _GoBack]STEP 8: Repeat steps 1 through 7 until process is completed, making sure to periodically check course line against a parallel reference line or course.
